**SPECIFICATION**

|  |  |
| --- | --- |
| Product | Tri-axle 42,000 liters fuel tanker trailer |
| **Weight & Size:** | |
| Loading capacity: | 42,000 Liters |
| Overall L\*W\*H: | 11,500\*2,550\*3,950 mm |
| Tare weight: | Around 7 tons |
| **Frame:** | |
| Material of main beam: | CIMC specified high strength steel |
| **Tanker Body:** | |
| Tanker body: | Material : aluminum alloy 5182. thickness:6mm, end plate:6mm |
| Manhole: | 5 pcs, aluminum alloy explosion-proof manhole, diameter: 20” |
| Compartment: | 5 pcs (the volume of each compartment could be designed according to customer’s requirement) |
| Discharge valve: | 5 units 3” aluminum API discharge valve |
| Emergency valve : | 5 units 4" pneumatic aluminum alloy emergency valve |
| Top handrail: | Collapsible type |
| Top walking way: | Aluminium top anti-sliding walkway |
| Discharge rubber hose: | 3 inch, 2 pcs |
| Discharge hose carrier: | 2pcs |
| Ladder: | One aluminum alloy front ladder |
| **Running Gear:** |  |
| Axle: | 3x13 tons axles , bpw brand |
| Tire: | 12R22.5 tubeless tires , 13 pcs,linglong brand(one spare included) |
| Suspension: | Mechanical suspension with 10 pcs spring leaf |
| Landing gear: | JOST E100 landing gear |
| Kingpin: | JOST 2 or 3.5 inch bolted type |
| **Brake system:** |  |
| Emergency relay valve | Wabco |
| Air tanker: | 2\*46L |
| Brake chamber: | Six-double structure brake chamber |
| ABS: | Equipped |
| **Electrical System:** |  |
| Receptacle: | 7-way socket standard |
| Voltage: | 24 Volt |
| Light: | LED |
| **Color:** | White paint with customized logo |
| **Accessories:** | 1 pcs tool box + 1 spare tire carrier |
|  | |